Shimmer Calibration

Program Shimmer with BTStreaming:

* Go to: C:\Users\310153563\Desktop\Shimmer\Download\Shimmer2 BSL
* Program with BTSTreaming

Got to

accel=1

gyro=0

mag=0

ecg=1

emg=0

gsr=0

anex7=0

anex0=0

str=0

heart=0

acc\_range=3

gs\_range=4

mg\_internal\_rate=7

mg\_range=1

user\_button\_enable=0

gyr\_button\_enable=0

PMUX\_enable=0

5V\_enable=0

sample\_rate=170.7

iammaster=0

sync=0

interval=120

timestamps=1

realtime=0

singletouch=0

myid=1

Nshimmer=1

shimmername=ecg

experimentid=ADLTest

configtime=1422268834